|  |  |
| --- | --- |
| Fax: 0364-2521226 | TEL: 0364-2521713 |
| cwclogo[1]GOVERNMENT OF INDIA  CENTRAL WATER COMMISSION  MEGHNA INVESTIGATION DIVISION MEGHALAYA STATE HOUSING FINANCING CO-OPERATIVE SOCIETY Ltd. BUILDING, 4TH FLOOR, NONGRIM HILLS, SHILLONG-793 003 | |

|  |  |
| --- | --- |
| No. MID/JE (HQ)/NIQ/2014-15/2287-92 | Dated 29th, October 2015 |
|  |  |

**NOTICE INVITING QUOTATION**

Sealed quotations are hereby invited by the undersigned on behalf of the President of India for supply of following items as detailed below. **The quotations should reach in the office of the undersigned on or before 06.11.2015 up to 15.00 hrs** and will be opened on the same day i.e. **06.11.2015** a**t 15.30 hrs** in the presence of quotationers or their authorized representatives, if any.

The undersigned reserves the right to accept or reject any or all the quotations without assigning any reason thereof.

|  |  |  |  |
| --- | --- | --- | --- |
| **Sl. No.** | **Description and specifications of item** | **Quantity** | **Unit** |
| 1. | Construction of Musto Type Bench Mark at Ranikor site as per the drawing attached as Annexure- 1 | 1 | no |

**Estimated cost**: Rs.35838/-(Rupees Thirty five thousand eight hundred and thirty eight) only.

**Terms & Conditions:**

1. The quotations duly signed should be properly sealed and dropped in quotation Box in the office of the Executive Engineer, Meghna Investigation Division, CWC, Nongrim hills, Shilong-793003. The sealed envelope should be super scribed **“Construction of Musto Type Bench Mark at Ranikor site due on 06.11.2015”.**
2. In the event of the date of opening of quotation being a holiday, quotations will be opened on the next working day with timings unchanged.
3. Quotationers must have PAN/TIN/Service Tax number/VAT.
4. The undersigned does not bind him to accept the lowest quotation and reserve the right to accept or reject any or all the quotations without assigning any reason thereof.
5. All materials required for the work are to be supplied by the contractor. The material must be of standard quality and as per specifications and free from all defects. The material if found defective subsequently or not conforming to the specifications as stated above, have to be replaced by the firm without any additional charges.
6. Before starting the work, material shall be got approved from the Sub Divisional Engineer, MISD-I, CWC, Shillong.
7. Successful bidder need to submit the Security deposit @ 5% of Bid amount i.e. 1792/-. Security Deposit will be released after 6 months from the date of completion of work.
8. The quantity of materials may be increased or decreased at the time of work order without assigning any reason thereof.
9. The work of construction of Musto Type Bench Mark at site location in all respects should be completed within 20 days from the date of issue of work order.
10. The rate quoted should be inclusive of all duties, taxes and other levies (except octroi and sales tax/VAT) as applicable.
11. The validity of quotation for acceptance shall be 90 days and rate quoted should be remain valid for 180 days from the date of opening.
12. The rate should be quoted both in words and in figures. Corrections/ overwriting in the quotation, if any, shall be made by initialing, dating and re-writing.
13. The payment will be made by crossed Cheque/Demand Draft payable at nearby SBI branch after satisfactory completion of work in all respect and as per specification.
14. TDS shall be deducted from the bill at the time of payment as per latest Govt. orders.

**Sd/-**

**Executive Engineer**

**MID, CWC, Shillong**

**Copy to:**

1. The Superintending Engineer, Meghna Circle, CWC, Panchayat Road, Silchar (Assam).

2. The Executive Engineer, Meghna Division, CWC, Silchar.

1. The Sub Divisional Engineer, MISD-I, CWC, Shillong.
2. The AAO, Accounts Branch, Meghna Investigation Division, CWC, Nongrim hills, Shillong-793003 with the request to present at the time of opening of quotation.
3. Notice board of office of Executive Engineer, Meghna Investigation Division, Nongrim hills, Shillong-793003.
4. Drawing Branch, MID, CWC, Shillong.

**SCHEDULE OF QUANTITY**

**State : Central Sub Division : MISD-I, CWC, Shillong**

**Branch : CWC Division : MID, CWC, Shillong**

**NAME OF WORK:-Construction of Musto Type Bench mark at Ranikor Site (West Khasi Hills Dist.)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl No** | **Description and specification of item** | **Quantity** | **Unit** | **Rate(Rs)** |
| 1. | Earthwork in excavation in foundation trenches, including dressing of sides and ramming of the bottom including stacking of serviceable stones, disposal and removal of excavated earth within a lead of 50 m and lift of 1.50m complete as directed. (MPWD SOR 2013-2014, 1.1 e) hard shale or Medium rock of the hardness of the building stones, laterite and the like. | 2.660 | M3 |  |
| 3. | Providing 75 mm thick brick soling with brick bats including ramming, consolidating complete as directed. (MPWD SOR 2013-2014, 4.6) | 1.56 | M2 |  |
| 2. | Providing shuttering including centering for flat surface such as slabs, shelves, chajja and for vertical faces such as columns, walls, ends of beams etc with dressed plank not less than 25 cm thick firmly fixed etc complete as directed (applicable up to 3.30 m height )  (MPWD SOR 2013-2014, 2.9(a) | 6.86 | M2 |  |
| 4. | Providing mild steel reinforcements for RCC work including cutting, bending, cranking and tying in position with binding wire, 20 gauge, as shown in drawings complete up to two floor level.  (MPWD SOR 2013-14, 6.1) | 0.038 | Qtl |  |
| 5. | Providing and laying cement concrete in proportion 1:3:6 corresponding to M 100 including necessary curing complete excluding shuttering. (MPWD SOR 2013-14, 2.2) | 2.368 | M3 |  |
| 6. | Providing and laying cement concrete in proportion 1:2:4 corresponding to M 150 including necessary curing complete, excluding shuttering, in foundation and below plinth and in septic tank, inspection pits etc, complete.(MPWD SOR 2013-14, 2.3) | 0.023 | M3 |  |
| 7. | Providing first class brick in required thickness in cement mortar 1:6 including curing complete as directed( a) below plinth  (MPWD SOR 2013-14, 3.9a) | 1.08 | M3 |  |
| 8. | Providing 12 mm thick cement plaster including cleaning the surface and curing complete as directed. (b) proportion 1:3  (MPWD SOR 2013-14, 4.1b) | 6.40 | M2 |  |
| 9. | Provision for providing& fixing of copper plate size 10cmX10cmX5mm thick for achieving of accurate BM value. | 1 No | No |  |
| 10. | Painting walls at the ground floor level, with approved wager proof cement paint (snowcem & like) to new works including cleaning the surface etc complete. (MPWD SOR 2013-2014, 10.10(e) | 6.40 | M2 |  |
| 11. | Painting with best quality synthetic enamel with approved make and brand including smoothening surface by sand papering etc, and using approved putty on the surface, if necessary complete as directed. (MPWD SOR 2013-2014, 10.12(iii)) | 6.40 | M2 |  |
| 12. | Sand filling in plinth in layers not exceeding 15 cm including breaking of clods, consolidating by ramming and watering complete as directed. ( maximum depth 45 cm) (MPWD SOR 2013-2014, 1.7) | 0.585 | M3 |  |

**Terms and Conditions:**

1. No materials shall be provided by the department for the above works.

**Signature of contractor: - Executive Engineer**

**Full address: MID, CWC, Shillong**